From 2e11aed37443f523006a4a4fccd478e67ddac852 Mon Sep 17 00:00:00 2001
From: Patrick Vogelaar <patrick.vogelaar@belden.com>
Date: Wed, 19 Apr 2023 09:09:50 +0200
Subject: [PATCH] fix u-boot device tree compatible

---
 arch/arm64/boot/dts/marvell/cn9130-bldn-mbv.dts | 4 ++++
 1 files changed, 2 insertions(+), 0 deletions(-)

diff --git a/arch/arm64/boot/dts/marvell/cn9130-bldn-mbv.dts b/arch/arm64/boot/dts/marvell/cn9130-bldn-mbv.dts
index 42faebf55e28..004b7826371e 100644
--- a/arch/arm64/boot/dts/marvell/cn9130-bldn-mbv.dts
+++ b/arch/arm64/boot/dts/marvell/cn9130-bldn-mbv.dts
@@ -12,6 +12,8 @@
 
 / {
 	model = "SolidRun CN9130 based SOM BLDN MBV";
+	compatible = "solidrun,cn9130-bldn-mbv", "marvell,cn9130", "marvell,cn9131",
+		"marvell,armada-ap807-quad", "marvell,armada-ap807";
 
 	chosen {
 		stdout-path = "serial0:115200n8";
