
SWUPDATE_IMAGES += "flash-image"
SWUPDATE_IMAGES_FSTYPES[flash-image] = ".bin"

COREOS_SWUPDATE_EXTENDS_FOR:append = "cn913x"

def coreos_swupdate_extends_images_for_cn913x(d,s):
    boot0 = {
        "filename" : "flash-image.bin",
        "installed-directly" : "true",
        "device" : "/dev/disk/by-partlabel/fw0",
        "type" : "raw",
        "sha256" : swupdate_get_sha256(d, s, "flash-image.bin"),
    }

    boot1 = boot0.copy()
    boot1["device"] = "/dev/disk/by-partlabel/fw1"


    return [boot0, boot1]
