label: gpt
device: /dev/mmcblk1
unit: sectors
first-lba: 34
last-lba: 7471070
sector-size: 512

# EBBR 2.1.0 section 4.1.1 mandate the use of an unused type UUID and to set
# the RequiredPartition label for part of the firmware stored in the main disk
# https://arm-software.github.io/ebbr/#section-gpt-parts
# next two type were generated
/dev/mmcblk1p1 : start=         256, size=         512, type=4DA6E9DA-C803-4BE4-BAC4-8192717C5EB0, name="mlo", attrs="RequiredPartition"
/dev/mmcblk1p2 : start=         768, size=        8192, type=5B97345D-B7A1-47D3-A491-ED40F4841639, name="uboot", attrs="RequiredPartition"

/dev/mmcblk1p3 : start=        8960, size=      131072, ${SFDISK_PART_EFI}
/dev/mmcblk1p4 : start=      140032, size=      262144, ${SFDISK_PART_EFIBOOTGUARD_A}
/dev/mmcblk1p5 : start=      402176, size=      262144, ${SFDISK_PART_EFIBOOTGUARD_B}
/dev/mmcblk1p6 : start=      664320, size=     3403375, ${SFDISK_PART_ROOT_A}
/dev/mmcblk1p7 : start=     4067695, size=     3403375, ${SFDISK_PART_ROOT_B}
