From 0017797ce718f4512271deddde75120c57623049 Mon Sep 17 00:00:00 2001
From: Samuel Dolt <samuel.dolt@netmodule.com>
Date: Tue, 24 Jan 2023 15:22:58 +0100
Subject: [PATCH] cn9130: fix compatible node inside dts

---
 arch/arm/dts/cn9130-bldn-mbv.dts | 7 ++++---
 arch/arm/dts/cn9130-cex7-A.dts   | 7 ++++---
 arch/arm/dts/cn9130-cf-pro.dts   | 7 ++++---
 3 files changed, 12 insertions(+), 9 deletions(-)

diff --git a/arch/arm/dts/cn9130-bldn-mbv.dts b/arch/arm/dts/cn9130-bldn-mbv.dts
index 9e10eab008..a91c490218 100644
--- a/arch/arm/dts/cn9130-bldn-mbv.dts
+++ b/arch/arm/dts/cn9130-bldn-mbv.dts
@@ -10,9 +10,10 @@
 
 / {
 	model = "Belden CN9130 based SOM and Carrier MBV-A/B";
-	compatible = "marvell,cn9130-db", "marvell,cn91xx", "marvell,cn9030-vd",
-		     "marvell,cn9030", "marvell,armada-ap806-quad",
-		     "marvell,armada-ap806", "marvell,armada70x0";
+	compatible =  "solidrun,cn9130-bldn-mbv", "marvell,cn9130-db",
+		"marvell,cn91xx", "marvell,cn9030-vd", "marvell,cn9030",
+		"marvell,armada-ap806-quad", "marvell,armada-ap806",
+		"marvell,armada70x0";
 
 	chosen {
 		stdout-path = "serial0:115200n8";
diff --git a/arch/arm/dts/cn9130-cex7-A.dts b/arch/arm/dts/cn9130-cex7-A.dts
index 209e485822..9995a586f6 100644
--- a/arch/arm/dts/cn9130-cex7-A.dts
+++ b/arch/arm/dts/cn9130-cex7-A.dts
@@ -10,9 +10,10 @@
 
 / {
 	model = "SolidRun CN9130 based COM express type 7";
-	compatible = "marvell,cn9130-db", "marvell,cn91xx", "marvell,cn9030-vd",
-		     "marvell,cn9030", "marvell,armada-ap806-quad",
-		     "marvell,armada-ap806", "marvell,armada70x0";
+	compatible =  "solidrun,cn9130-cex7", "marvell,cn9130-db",
+		"marvell,cn91xx", "marvell,cn9030-vd", "marvell,cn9030",
+		"marvell,armada-ap806-quad", "marvell,armada-ap806",
+		"marvell,armada70x0";
 
 	chosen {
 		stdout-path = "serial0:115200n8";
diff --git a/arch/arm/dts/cn9130-cf-pro.dts b/arch/arm/dts/cn9130-cf-pro.dts
index 6931818cf6..dae7a75076 100644
--- a/arch/arm/dts/cn9130-cf-pro.dts
+++ b/arch/arm/dts/cn9130-cf-pro.dts
@@ -10,9 +10,10 @@
 
 / {
 	model = "SolidRun CN9130 based SOM ClearFog Pro";
-	compatible = "marvell,cn9130-db", "marvell,cn91xx", "marvell,cn9030-vd",
-		     "marvell,cn9030", "marvell,armada-ap806-quad",
-		     "marvell,armada-ap806", "marvell,armada70x0";
+	compatible = "solidrun,cn9130-cf-pro", "marvell,cn9130-db",
+		"marvell,cn91xx", "marvell,cn9030-vd", "marvell,cn9030",
+		"marvell,armada-ap806-quad", "marvell,armada-ap806",
+		"marvell,armada70x0";
 
 	chosen {
 		stdout-path = "serial0:115200n8";
