# meta-netmodule-coreos-bsp

BSP layer for NetModule board

This layer depends on:

- meta-ti-bsp
- meta-arm

## SoC Family

This layer contains all CoreOS supported board manufactured by NetModule

## Availables Machines

This layer contains the following machine configuration:

### Based on the Gemini platform

- netmodule-hw34 (Codename for XG900)

**remarks**: Gemini based board use a TI am64xx (k3) family has a separate
R5 core that use another architecture as the main core, so for each machine you
will find a companion machine name `${MACHINE}-k3r5`. This config should not be
used as is, but will be automatically used for some recipes under the hood when
using `${MACHINE}` using Bitbake multiconfig feature.
