From 7e4c3c48c4ed9dcecf5228c6b4480a7c01fc6dca Mon Sep 17 00:00:00 2001
From: Samuel Dolt <samuel.dolt@netmodule.com>
Date: Tue, 19 Jul 2022 11:21:37 +0200
Subject: [PATCH] octeontx2_cn913x: increase CONFIG_SYS_BOOTM_LEN to 32MB

---
 include/configs/octeontx2_cn913x.h | 2 ++
 1 file changed, 2 insertions(+)

diff --git a/include/configs/octeontx2_cn913x.h b/include/configs/octeontx2_cn913x.h
index d01644fcb5..9edf57c6c2 100644
--- a/include/configs/octeontx2_cn913x.h
+++ b/include/configs/octeontx2_cn913x.h
@@ -22,6 +22,8 @@
 #define CONFIG_SYS_NAND_ONFI_DETECTION
 #define CONFIG_SYS_NAND_USE_FLASH_BBT
 
+#define CONFIG_SYS_BOOTM_LEN 0x3200000 /* 32MB */
+
 #define CONFIG_USB_MAX_CONTROLLER_COUNT (3 + 3)
 
 #define BOOT_TARGET_DEVICES(func) \
