From 03297ee2679e39da71dd39fb3076b305621c45d5 Mon Sep 17 00:00:00 2001
From: Josua Mayer <josua@solid-run.com>
Date: Tue, 22 Mar 2022 11:09:06 +0200
Subject: [PATCH] octeontx2_cn913x: remove console variable

console is now properly selected by chosen nodei n device-tree rather
than through bootargs.

Signed-off-by: Josua Mayer <josua@solid-run.com>
---
 include/configs/octeontx2_cn913x.h | 4 ----
 1 file changed, 4 deletions(-)

diff --git a/include/configs/octeontx2_cn913x.h b/include/configs/octeontx2_cn913x.h
index aa966bd292..d01644fcb5 100644
--- a/include/configs/octeontx2_cn913x.h
+++ b/include/configs/octeontx2_cn913x.h
@@ -8,9 +8,6 @@
 #ifndef _CONFIG_OCTEONTX2_CN913X_H
 #define _CONFIG_OCTEONTX2_CN913X_H
 
-#define CONFIG_DEFAULT_CONSOLE		"console=ttyS0,115200 "\
-					"earlycon=uart8250,mmio32,0xf0512000"
-
 #include <configs/mvebu_armada-common.h>
 
 /*
@@ -39,7 +36,6 @@
 
 #undef CONFIG_EXTRA_ENV_SETTINGS
 #define CONFIG_EXTRA_ENV_SETTINGS \
-	"console=" CONFIG_DEFAULT_CONSOLE "\0"\
 	"kernel_addr_r=0x7000000\0" \
 	"fdt_addr_r=0x6f00000\0" \
 	"ramdisk_addr_r=0x9000000\0" \
